2025-01-01

Run the SdErrorCode example to produce an updated list.

Code,Symbol - failed operation
0X00,SD_CARD_ERROR_NONE - No error
0X01,SD_CARD_ERROR_CMD0 - Card reset failed
0X02,SD_CARD_ERROR_CMD2 - SDIO read CID
0X03,SD_CARD_ERROR_CMD3 - SDIO publish RCA
0X04,SD_CARD_ERROR_CMD6 - Switch card function
0X05,SD_CARD_ERROR_CMD7 - SDIO card select
0X06,SD_CARD_ERROR_CMD8 - Send and check interface settings
0X07,SD_CARD_ERROR_CMD9 - Read CSD data
0X08,SD_CARD_ERROR_CMD10 - Read CID data
0X09,SD_CARD_ERROR_CMD12 - Stop multiple block transmission
0X0A,SD_CARD_ERROR_CMD13 - Read card status
0X0B,SD_CARD_ERROR_CMD17 - Read single block
0X0C,SD_CARD_ERROR_CMD18 - Read multiple blocks
0X0D,SD_CARD_ERROR_CMD24 - Write single block
0X0E,SD_CARD_ERROR_CMD25 - Write multiple blocks
0X0F,SD_CARD_ERROR_CMD32 - Set first erase block
0X10,SD_CARD_ERROR_CMD33 - Set last erase block
0X11,SD_CARD_ERROR_CMD38 - Erase selected blocks
0X12,SD_CARD_ERROR_CMD58 - Read OCR register
0X13,SD_CARD_ERROR_CMD59 - Set CRC mode
0X14,SD_CARD_ERROR_ACMD6 - Set SDIO bus width
0X15,SD_CARD_ERROR_ACMD13 - Read extended status
0X16,SD_CARD_ERROR_ACMD23 - Set pre-erased count
0X17,SD_CARD_ERROR_ACMD41 - Activate card initialization
0X18,SD_CARD_ERROR_ACMD51 - Read SCR data
0X19,SD_CARD_ERROR_READ_TOKEN - Bad read data token
0X1A,SD_CARD_ERROR_READ_CRC - Read CRC error
0X1B,SD_CARD_ERROR_READ_FIFO - SDIO fifo read timeout
0X1C,SD_CARD_ERROR_READ_REG - Read CID or CSD failed.
0X1D,SD_CARD_ERROR_READ_START - Bad readStart argument
0X1E,SD_CARD_ERROR_READ_TIMEOUT - Read data timeout
0X1F,SD_CARD_ERROR_STOP_TRAN - Multiple block stop failed
0X20,SD_CARD_ERROR_TRANSFER_COMPLETE - SDIO transfer complete
0X21,SD_CARD_ERROR_WRITE_DATA - Write data not accepted
0X22,SD_CARD_ERROR_WRITE_FIFO - SDIO fifo write timeout
0X23,SD_CARD_ERROR_WRITE_START - Bad writeStart argument
0X24,SD_CARD_ERROR_WRITE_PROGRAMMING - Flash programming
0X25,SD_CARD_ERROR_WRITE_TIMEOUT - Write timeout
0X26,SD_CARD_ERROR_DMA - DMA transfer failed
0X27,SD_CARD_ERROR_ERASE - Card did not accept erase commands
0X28,SD_CARD_ERROR_ERASE_SINGLE_SECTOR - Card does not support erase
0X29,SD_CARD_ERROR_ERASE_TIMEOUT - Erase command timeout
0X2A,SD_CARD_ERROR_INIT_NOT_CALLED - Card has not been initialized
0X2B,SD_CARD_ERROR_ADD_PIO_PROGRAM - Add PIO program
0X2C,SD_CARD_ERROR_INVALID_CARD_CONFIG - Invalid card config
0X2D,SD_CARD_ERROR_FUNCTION_NOT_SUPPORTED - Unsupported SDIO command
0X2E,SD_CARD_ERROR_UNKNOWN - Unknown error
